**AUTOMATIC FOLDER GLUER COUNTER EJECTOR (UP LIFT)**

|  |  |  |
| --- | --- | --- |
| Model | AFG-M-1200x2000 | AFG-M-1200x2400 |
|  Power consumption(Voltage, HZ) |  380V or 415 V, 50HZ, 3 phase |  380V or 415 V, 50HZ, 3 phase |
|  Max. carton box (L x W) |  500x500x500x500 |  600x600x600x600 |
|  Min. carton box (L x W) |  120x120x120x120(mini beam) |  120x120x120x120 mini beam |
|  200x200x200x200(big beam) |  200x200x200x200(big beam) |
|  Paperboard thickness |  2-9mm |  2-9mm |
|  Glue width |  45mm |  45mm |
|  Feeding mode |  Suction belt feeding |  Suction belt feeding |
|  Max. paperboard  (L x W) |  1200x2400 mm |  1200x2400 mm |
|  Min. paperboard (L x W) |  250x550mm  (mini beam) 300x800 mm  ( big beam) |  250x550mm  (mini beam) 300x800 mm  (big beam) |
|  Forming mode |  Up folding |  Up folding |
|  Total power (KW) |  12  |  12    |
|  Working speed pcs/min |  80-150 (by size and quality) |  80-150(by size and quality) |
|  Machine dimension |  8000x2800x1100 |  8000x3500x1100 |