**AUTOMATIC FOLDER GLUER COUNTER EJECTOR (UP LIFT)**

|  |  |  |
| --- | --- | --- |
| Model | AFG-M-1200x2000 | AFG-M-1200x2400 |
| Power consumption(Voltage, HZ) | 380V or 415 V, 50HZ, 3 phase | 380V or 415 V, 50HZ, 3 phase |
| Max. carton box (L x W) | 500x500x500x500 | 600x600x600x600 |
| Min. carton box (L x W) | 120x120x120x120(mini beam) | 120x120x120x120 mini beam |
| 200x200x200x200(big beam) | 200x200x200x200(big beam) |
| Paperboard thickness | 2-9mm | 2-9mm |
| Glue width | 45mm | 45mm |
| Feeding mode | Suction belt feeding | Suction belt feeding |
| Max. paperboard  (L x W) | 1200x2400 mm | 1200x2400 mm |
| Min. paperboard (L x W) | 250x550mm  (mini beam)  300x800 mm  ( big beam) | 250x550mm  (mini beam)  300x800 mm  (big beam) |
| Forming mode | Up folding | Up folding |
| Total power (KW) | 12 | 12 |
| Working speed pcs/min | 80-150 (by size and quality) | 80-150(by size and quality) |
| Machine dimension | 8000x2800x1100 | 8000x3500x1100 |